**Installation Instructions**

**Mat Preparation**

Before unrolling mat, allow mat to reach room temperature.

Unroll and place on smooth surface to allow mat to relax for a minimum of 24 hours.

**Location**

Select a smooth, level surface between the dirty area and the clean area you wish to protect. Place the mat where foot and wheel traffic will cross the mat.

**Surface Preparation**

After selecting a smooth level flat location for installation, thoroughly clean the surface of the existing floor. Sweep away loose dirt, mop and let fully dry. If wax is present on the floor, then completely strip wax from floor where mat is to be applied.

**Installation**

Remove liner covering the adhesive strips and apply the mat to the flat surface face down. Peel off the surface liner slowly. With two people lift and flip mat. Starting at one edge and working to the opposite edge, slowly apply mat to the floor. Immediately after mat has been applied to floor; clean mat (see reverse side for instructions). Mat is now ready to use.

It is strongly recommended to apply a bead of silicone caulk around the perimeter of the mat after installed to prevent water from seeping and collecting under the mat when cleaning. If water accumulates under the mat, mold can develop between the mat and the floor.

**Forktrucks**

Do not turn forklift truck wheels while on the mat. This will cause mat to tear.